**Planned Deviation Documentation**

|  |  |
| --- | --- |
| Site(s): | AHC - all Sites |
| Procedure: | QC frequency by Sysmex XN and XS System |
| Reason for Deviation: | Manufacturer (Sysmex) is having supply issues with QC: Instead of running QC twice per shift, we will be running it once per day. (POST shut down)Directions to turn off alarm for QC on the analyzer:1. Main Menu
2. IPU Settings
3. QC
4. QC Alarm
5. QC Alarm Setting
6. Un-click and change settings as needed. APPLY.

Sysmex Body Fluid Controls will only be run once per day of patient testing. |
| Medical Director or Designee: | Dr. Cacciabeve (*electronic signature*) & Dr. Beltaifa | Date:1/12/22 |
| Supervisor: | Hollie Genser & Zanetta Morrow | Date:1/12/22 |
| Deviation Start Date: | 1.12.22 | Deviation End Date: TBD |
|  |  |  |  |  |
| Testing Personnel Signatures | Start Deviation Signatures |  | End Deviation Signatures |  |
| Printed Name / Tech Code | Signature | Date | Signature | Date |
|  | *Captured via MTS update* |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |