**Planned Deviation Documentation**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Site(s): | AHC - all Sites | | | |
| Procedure: | QC frequency by Sysmex XN and XS System | | | |
| Reason for Deviation: | Manufacturer (Sysmex) is having supply issues with QC: Instead of running QC twice per shift, we will be running it once per day. (POST shut down)  Directions to turn off alarm for QC on the analyzer:   1. Main Menu 2. IPU Settings 3. QC 4. QC Alarm 5. QC Alarm Setting 6. Un-click and change settings as needed. APPLY.   Sysmex Body Fluid Controls will only be run once per day of patient testing. | | | |
| Medical Director or Designee: | Dr. Cacciabeve (*electronic signature*) & Dr. Beltaifa | | Date:1/12/22 | |
| Supervisor: | Hollie Genser & Zanetta Morrow | | Date:1/12/22 | |
| Deviation Start Date: | 1.12.22 | | Deviation End Date: TBD | |
|  |  |  |  |  |
| Testing Personnel Signatures | Start Deviation Signatures |  | End Deviation Signatures |  |
| Printed Name / Tech Code | Signature | Date | Signature | Date |
|  | *Captured via MTS update* |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |