#### Disconnecting and Reconnecting IPU to Host Computer on the Sysmex XN Hematology Analyzer

|  |  |  |
| --- | --- | --- |
| Background | This procedure describes how to disconnect and reconnect the IPU from the Host Computer during LIS downtime to ensure continuous operation of the Sysmex analyzer |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Procedure A | Follow the steps below to disconnect IPU from Host Computer

|  |  |
| --- | --- |
| Step | Action |
| 1 | On IPU Main menu, select Log off icon |
| 2 | Click Yes when prompted to log off |
| 3 | Enter username info: admin |
| 4 | Enter password info: m116m |
| 5 | Click OK |
| 6 | On IPU Main Menu, click IPU setting icon |
| 7 | In IPU setting display screen , under Connect option, select Host Computer |
| 8 |  In Host computer connection setting display screen, click “Host Computer Connection” box to remove check mark |
| 9 | Click OK to save changes and disconnect IPU from Host Computer**Note: Host computer status indicator light turns green to gray** |

  |

 Continued on next page

Disconnecting and Reconnecting IPU to Host Computer on the Sysmex XN Hematology Analyzer, Continued

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Procedure B | Follow the steps below to reconnect IPU to Host Computer

|  |  |
| --- | --- |
| Step | Action |
| 1 | On IPU Main menu, select Log off icon |
| 2 | Click Yes when prompted to log off |
| 3 | Enter username info: admin |
| 4 | Enter password info: m116m |
| 5 | Click OK |
| 6 | On IPU Main Menu, click IPU setting icon |
| 7 | In IPU setting display screen, under Connect option, select Host Computer |
| 8 | In Host computer connection setting display screen, click empty “Host Computer Connection” box to insert check mark |
| 9 | Click OK to save changes and reconnect IPU to Host Computer**Note: Host computer status indicator light turns gray to green** |

  |

|  |  |
| --- | --- |
| References | * Sysmex XN series Operator’s manual, March 2017
 |

 *End*