**C**

**Control Line ►C**

Analyzer checks for presence of the control line to confirm cassette integrity.

**Test Line ►T**

Development of this line represents the intensity line of a patient sample or control based upon the amount of hCG present in the urine.

**Reference Line ►R**

Line intensity is anchored toreflect a level for positiveresult comparison.