**Helmer Quickthaw Preventive Maintenance Form**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Weekly Maintenance**  Drain and clean the interior and exterior of the thawer, and refill with clean water and bacterial growth inhibitor. | **Date** | **Date** | **Date** | **Date** | **Date** | **Review by/ date** |
| Controller Temp/Digital Temp |  |  |  |  |  |  |
| Water changed & cleaned / √ |  |  |  |  |  |  |
| Tech ID / Date & time |  |  |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Quarterly Maintenance** | **Date 1Qtr** | **Date 2Qtr** | **Date 3Qtr** | **Date 4Qtr** | **Done/**  **OK** | **Tech ID** | **Review by/date** |
| 2. Lubricate the moving  parts (baskets and  rails) |  |  |  |  |  |  |  |
| 3. Check the bearings  for wear. |  |  |  |  |  |  |  |

Additional actions needed/taken:

Date/ Tech ID

.