**Helmer Quickthaw Preventive Maintenance Form**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Weekly Maintenance**Drain and clean the interior and exterior of the thawer, clean vents, and refill with clean water and bacterial growth inhibitor. | **Date** | **Date** | **Date** | **Date** | **Date** | **Review by/date** |
| Controller Temp/Digital Temp |  |  |  |  |  |  |
| Water changed & cleaned / √ |  |  |  |  |  |  |
| Tech ID / Date & time |  |  |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Quarterly Maintenance** | **Date 1Qtr** | **Date 2Qtr**  | **Date 3Qtr**  | **Date 4Qtr**  | **Done/****OK** | **Tech ID** | **Review by/date** |
| Test High Temperature |  |  |  |  |  |  |  |
| Check temperature calibration for controller readout |  |  |  |  |  |  |  |

Additional actions needed/taken:

 Date/ Tech ID

.