2015 Quiz for Radiometer Annual competency

Name: Date:

1. A red light on the instrument panel means:
2. The instrument is in standby
3. The instrument has a problem and cannot be used until it is resolved
4. Nothing, it is always red
5. Quality control must be run:
6. at all changes in reagent,
7. changes of the sensor cassette
8. Each day of use
9. All of the above
10. What does the red flag in these results mean?



1. What does it mean when the results have a “!!” instead of a result?
2. The last manual QC sample run on this parameter was outside the acceptable range.
3. The final result is outside the measuring range of the analyzer.
4. Possible air was identified in either the sample or the flush during analysis.

Signature: